{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":18,"n_cols":4,"rows_kept":18,"cut":false,"hidden":false,"merged":[[0,0,0,3],[4,2,4,3],[16,2,16,3],[2,0,19,0]]}
["附表3-1 YEAR年ROAD高速公路养护质量目标表(PWI)"]
["目标分项","目标细项","现状内容","目标内容"]
["养护质量","1、公路技术状况指数MQI ",{"$f":"IF(ISERROR((C14*0.08)),0,(C14*0.08))+IF(ISERROR((C6*0.7)),0,(C6*0.7))+IF(ISERROR((C15*0.12)),0,(C15*0.12))+IF(ISERROR((C16*0.1)),0,(C16*0.1))","v":0}]
[null,"2、次差路率"]
[null,"3、各分项性能指数"]
[null,"3.1路面使用性能指数PQI",{"$f":"IF(ISERROR((C7*0.35)),0,(C7*0.35))+IF(ISERROR((C8*0.3)),0,(C8*0.3))+IF(ISERROR((C9*0.15)),0,(C9*0.15))+IF(ISERROR((C10*0.1)),0,(C10*0.1))+IF(ISERROR((C11*0.1)),0,(C11*0.1))","v":0}]
[null,"3.1.1 路面损坏状况指数PCI"]
[null,"3.1.2 路面行驶质量指数RQI"]
[null,"3.1.3 路面车辙深度指数RDI"]
[null,"3.1.4 路面跳车指数PBI"]
[null,"3.1.5路面磨耗指数PWI"]
[null,"3.1.6路面抗滑性能指数SRI"]
[null,"3.1.7路面结构强度指数PSSI"]
[null,"3.2路基技术状况指数SCI"]
[null,"3.3桥涵构造物技术状况指数BCI"]
[null,"3.4沿线设施技术状况指数TCI"]
[null,"3.5桥梁技术状况"]
[null,"一、二类桥梁所占比例（%）"]